(kicad_pcb (version 4) (host pcbnew 4.0.2-4+6225~38~ubuntu15.10.1-stable)
  (general
    (links 21)
    (no_connects 0)
    (area 191.95 31.60488 276.910001 133.400001)
    (thickness 1.6)
    (drawings 4)
    (tracks 80)
    (zones 0)
    (modules 13)
    (nets 17)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.25)
    (user_trace_width 1.3)
    (user_trace_width 10)
    (trace_clearance 0.25)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.25)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(AC1-Pad1)")
  (net 2 "Net-(AC1-Pad2)")
  (net 3 "Net-(AC2-Pad1)")
  (net 4 "Net-(AC2-Pad2)")
  (net 5 "Net-(AC3-Pad1)")
  (net 6 "Net-(AC3-Pad2)")
  (net 7 "Net-(P1-Pad1)")
  (net 8 "Net-(P1-Pad2)")
  (net 9 "Net-(P1-Pad3)")
  (net 10 "Net-(P1-Pad4)")
  (net 11 "Net-(R1-Pad1)")
  (net 12 "Net-(R2-Pad1)")
  (net 13 "Net-(R3-Pad1)")
  (net 14 "Net-(U1-Pad4)")
  (net 15 "Net-(U3-Pad4)")
  (net 16 "Net-(U4-Pad4)")
  (net_class Default "This is the default net class."
    (clearance 0.25)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(P1-Pad1)")
    (add_net "Net-(P1-Pad2)")
    (add_net "Net-(P1-Pad3)")
    (add_net "Net-(P1-Pad4)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(R3-Pad1)")
    (add_net "Net-(U1-Pad4)")
    (add_net "Net-(U3-Pad4)")
    (add_net "Net-(U4-Pad4)")
  )
  (net_class BUS ""
    (clearance 0.8)
    (trace_width 10)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (net_class Channel ""
    (clearance 0.4)
    (trace_width 1.3)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(AC1-Pad1)")
    (add_net "Net-(AC1-Pad2)")
    (add_net "Net-(AC2-Pad1)")
    (add_net "Net-(AC2-Pad2)")
    (add_net "Net-(AC3-Pad1)")
    (add_net "Net-(AC3-Pad2)")
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM7mm placed (layer F.Cu) (tedit 569FCF07)
    (at 228.6 118.11)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference R2 (at 4.05892 -3.50012) (layer F.SilkS))
    (fp_text value 330R (at 3.81 3.81) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 12 "Net-(R2-Pad1)"))
    (pad 2 thru_hole circle (at 7.62 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 9 "Net-(P1-Pad3)"))
  )
  (module Housings_DIP:DIP-6_W7.62mm_LongPads placed (layer F.Cu) (tedit 54130A77)
    (at 228.6 114.3 90)
    (descr "6-lead dip package, row spacing 7.62 mm (300 mils), longer pads")
    (tags "dil dip 2.54 300")
    (fp_text reference U3 (at 0 -5.22 90) (layer F.SilkS))
    (fp_text value MOC3023M (at 0 -3.72 90) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(R2-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(P1-Pad1)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS))
    (pad 4 thru_hole oval (at 7.62 5.08 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(U3-Pad4)"))
    (pad 5 thru_hole oval (at 7.62 2.54 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS))
    (pad 6 thru_hole oval (at 7.62 0 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(AC2-Pad2)"))
    (model Housings_DIP.3dshapes/DIP-6_W7.62mm_LongPads.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04 placed (layer F.Cu) (tedit 0)
    (at 233.68 57.15)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at 0 -5.1) (layer F.SilkS))
    (fp_text value CONN_01X04 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(P1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(P1-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(P1-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(P1-Pad4)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x04.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module TO_SOT_Packages_THT:TO-220_Neutral123_Horizontal_LargePads (layer F.Cu) (tedit 0)
    (at 231.14 100.33)
    (descr "TO-220, Neutral, Horizontal, Large Pads,")
    (tags "TO-220, Neutral, Horizontal, Large Pads,")
    (fp_text reference U5 (at 0.24892 -22.84984) (layer F.SilkS))
    (fp_text value TRIAC (at -0.20066 4.24942) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 0 90) (size 3.50012 1.69926) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(AC2-Pad2)"))
    (pad 1 thru_hole oval (at -2.54 0 90) (size 3.50012 1.69926) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(AC2-Pad1)"))
    (pad 3 thru_hole oval (at 2.54 0 90) (size 3.50012 1.69926) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(U3-Pad4)"))
    (pad "" np_thru_hole circle (at 0 -16.764 90) (size 3.79984 3.79984) (drill 3.79984) (layers *.Cu *.Mask F.SilkS))
    (model TO_SOT_Packages_THT.3dshapes/TO-220_Neutral123_Horizontal_LargePads.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connect:AK300-2 placed (layer F.Cu) (tedit 54792136)
    (at 200.66 69.85 90)
    (descr CONNECTOR)
    (tags CONNECTOR)
    (attr virtual)
    (fp_text reference AC1 (at -1.92 -6.985 90) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 2.779 7.747 90) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0 90) (size 1.9812 3.9624) (drill 1.3208) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 1 "Net-(AC1-Pad1)"))
    (pad 2 thru_hole oval (at 5 0 90) (size 1.9812 3.9624) (drill 1.3208) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 2 "Net-(AC1-Pad2)"))
  )
  (module Connect:AK300-2 placed (layer F.Cu) (tedit 54792136)
    (at 200.66 83.82 90)
    (descr CONNECTOR)
    (tags CONNECTOR)
    (attr virtual)
    (fp_text reference AC2 (at -1.92 -6.985 90) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 2.779 7.747 90) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0 90) (size 1.9812 3.9624) (drill 1.3208) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 3 "Net-(AC2-Pad1)"))
    (pad 2 thru_hole oval (at 5 0 90) (size 1.9812 3.9624) (drill 1.3208) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 4 "Net-(AC2-Pad2)"))
  )
  (module Connect:AK300-2 placed (layer F.Cu) (tedit 54792136)
    (at 200.66 97.79 90)
    (descr CONNECTOR)
    (tags CONNECTOR)
    (attr virtual)
    (fp_text reference AC3 (at -1.92 -6.985 90) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 2.779 7.747 90) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0 90) (size 1.9812 3.9624) (drill 1.3208) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 5 "Net-(AC3-Pad1)"))
    (pad 2 thru_hole oval (at 5 0 90) (size 1.9812 3.9624) (drill 1.3208) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 6 "Net-(AC3-Pad2)"))
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM7mm placed (layer F.Cu) (tedit 569FCF07)
    (at 215.9 36.83)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference R1 (at 4.05892 -3.50012) (layer F.SilkS))
    (fp_text value 330R (at 3.81 3.81) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 11 "Net-(R1-Pad1)"))
    (pad 2 thru_hole circle (at 7.62 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 10 "Net-(P1-Pad4)"))
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM7mm placed (layer F.Cu) (tedit 569FCF07)
    (at 210.82 118.11)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference R3 (at 4.05892 -3.50012) (layer F.SilkS))
    (fp_text value 330R (at 3.81 3.81) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 13 "Net-(R3-Pad1)"))
    (pad 2 thru_hole circle (at 7.62 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 8 "Net-(P1-Pad2)"))
  )
  (module Housings_DIP:DIP-6_W7.62mm_LongPads placed (layer F.Cu) (tedit 54130A77)
    (at 215.9 40.64 270)
    (descr "6-lead dip package, row spacing 7.62 mm (300 mils), longer pads")
    (tags "dil dip 2.54 300")
    (fp_text reference U1 (at 0 -5.22 270) (layer F.SilkS))
    (fp_text value MOC3023M (at 0 -3.72 270) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0 270) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(R1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(P1-Pad1)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS))
    (pad 4 thru_hole oval (at 7.62 5.08 270) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(U1-Pad4)"))
    (pad 5 thru_hole oval (at 7.62 2.54 270) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS))
    (pad 6 thru_hole oval (at 7.62 0 270) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(AC1-Pad2)"))
    (model Housings_DIP.3dshapes/DIP-6_W7.62mm_LongPads.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-220_Neutral123_Horizontal_LargePads (layer F.Cu) (tedit 0)
    (at 213.36 57.15 180)
    (descr "TO-220, Neutral, Horizontal, Large Pads,")
    (tags "TO-220, Neutral, Horizontal, Large Pads,")
    (fp_text reference U2 (at 0.24892 -22.84984 180) (layer F.SilkS))
    (fp_text value TRIAC (at -0.20066 4.24942 180) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 0 270) (size 3.50012 1.69926) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(AC1-Pad2)"))
    (pad 1 thru_hole oval (at -2.54 0 270) (size 3.50012 1.69926) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(AC1-Pad1)"))
    (pad 3 thru_hole oval (at 2.54 0 270) (size 3.50012 1.69926) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(U1-Pad4)"))
    (pad "" np_thru_hole circle (at 0 -16.764 270) (size 3.79984 3.79984) (drill 3.79984) (layers *.Cu *.Mask F.SilkS))
    (model TO_SOT_Packages_THT.3dshapes/TO-220_Neutral123_Horizontal_LargePads.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-6_W7.62mm_LongPads placed (layer F.Cu) (tedit 54130A77)
    (at 210.82 114.3 90)
    (descr "6-lead dip package, row spacing 7.62 mm (300 mils), longer pads")
    (tags "dil dip 2.54 300")
    (fp_text reference U4 (at 0 -5.22 90) (layer F.SilkS))
    (fp_text value MOC3023M (at 0 -3.72 90) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(R3-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(P1-Pad1)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS))
    (pad 4 thru_hole oval (at 7.62 5.08 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(U4-Pad4)"))
    (pad 5 thru_hole oval (at 7.62 2.54 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS))
    (pad 6 thru_hole oval (at 7.62 0 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(AC3-Pad2)"))
    (model Housings_DIP.3dshapes/DIP-6_W7.62mm_LongPads.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-220_Neutral123_Horizontal_LargePads (layer F.Cu) (tedit 0)
    (at 213.36 100.33)
    (descr "TO-220, Neutral, Horizontal, Large Pads,")
    (tags "TO-220, Neutral, Horizontal, Large Pads,")
    (fp_text reference U6 (at 0.24892 -22.84984) (layer F.SilkS))
    (fp_text value TRIAC (at -0.20066 4.24942) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 0 90) (size 3.50012 1.69926) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(AC3-Pad2)"))
    (pad 1 thru_hole oval (at -2.54 0 90) (size 3.50012 1.69926) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(AC3-Pad1)"))
    (pad 3 thru_hole oval (at 2.54 0 90) (size 3.50012 1.69926) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(U4-Pad4)"))
    (pad "" np_thru_hole circle (at 0 -16.764 90) (size 3.79984 3.79984) (drill 3.79984) (layers *.Cu *.Mask F.SilkS))
    (model TO_SOT_Packages_THT.3dshapes/TO-220_Neutral123_Horizontal_LargePads.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 276.86 35.56) (end 193.04 35.56) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 193.04 133.35) (end 193.04 35.56) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 276.86 133.35) (end 193.04 133.35) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 276.86 35.56) (end 276.86 133.35) (angle 90) (layer Edge.Cuts) (width 0.1))
)
