(kicad_pcb (version 4) (host pcbnew 4.0.1-stable)
  (general
    (links 42)
    (no_connects 0)
    (area 14.225001 18.339999 50.656441 45.245001)
    (thickness 1.6)
    (drawings 8)
    (tracks 169)
    (zones 0)
    (modules 25)
    (nets 15)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.4)
    (trace_clearance 0.4)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.4)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.7)
    (via_drill 0.5)
    (via_min_size 0.65)
    (via_min_drill 0.5)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.3)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 0.5 0.5)
    (mod_text_width 0.075)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 24.765 18.415)
    (grid_origin 24.765 18.415)
    (visible_elements FFFFFEFF)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions true)
      (excludeedgelayer false)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin true)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk true)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory output/))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 "Net-(C1-Pad2)")
  (net 3 "Net-(C2-Pad1)")
  (net 4 "Net-(C2-Pad2)")
  (net 5 "Net-(C3-Pad1)")
  (net 6 Earth)
  (net 7 "Net-(C4-Pad1)")
  (net 8 "Net-(C5-Pad2)")
  (net 9 "Net-(C6-Pad1)")
  (net 10 "Net-(C7-Pad1)")
  (net 11 "Net-(D1-Pad2)")
  (net 12 "Net-(L2-Pad1)")
  (net 13 "Net-(P1-Pad1)")
  (net 14 +5V)
  (net_class Default "This is the default net class."
    (clearance 0.4)
    (trace_width 0.4)
    (via_dia 0.7)
    (via_drill 0.5)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net Earth)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C5-Pad2)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(L2-Pad1)")
    (add_net "Net-(P1-Pad1)")
  )
  (module Capacitors_SMD:C_0603_HandSoldering placed (layer F.Cu) (tedit 56EABEA9)
    (at 35.875 29.845 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C6 (at -0.574 -1.27 180) (layer F.SilkS))
    (fp_text value 4.7pF (at 0.635 1.27 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C6-Pad1)"))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering placed (layer F.Cu) (tedit 56EABDF2)
    (at 26.67 37 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R8 (at -2.583 0 270) (layer F.SilkS))
    (fp_text value 3k (at 1.1 1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C7-Pad1)"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 Earth))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:c_elec_6.3x5.7 placed (layer F.Cu) (tedit 56EABEF8)
    (at 29.464 29.63418 270)
    (descr "SMT capacitor, aluminium electrolytic, 6.3x5.7")
    (attr smd)
    (fp_text reference C7 (at 0 0.254 360) (layer F.SilkS))
    (fp_text value 10uF (at 0 -1.27 270) (layer F.Fab))
    (pad 1 smd rect (at 2.75082 0 270) (size 3.59918 1.6002) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C7-Pad1)"))
    (pad 2 smd rect (at -2.75082 0 270) (size 3.59918 1.6002) (layers F.Cu F.Paste F.Mask)
      (net 6 Earth))
    (model Capacitors_SMD.3dshapes/c_elec_6.3x5.7.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering placed (layer F.Cu) (tedit 56EABE0E)
    (at 28.575 37.15 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at 2.22 0 270) (layer F.SilkS))
    (fp_text value 1.7pF (at 0.955 1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 6 Earth))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering placed (layer F.Cu) (tedit 56EABF3A)
    (at 32.385 36.83 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference L3 (at 2.667 0 90) (layer F.SilkS))
    (fp_text value 5nH (at 0.635 -1.27 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 14 +5V))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering placed (layer B.Cu) (tedit 56EABEA1)
    (at 29.845 34.925 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R7 (at -0.508 -1.27 180) (layer B.SilkS))
    (fp_text value 100R (at 0.465 1.27 180) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 14 +5V))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(C7-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering placed (layer B.Cu) (tedit 56EABE93)
    (at 29.718 31.75 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at -0.127 -1.143 180) (layer B.SilkS))
    (fp_text value 3k (at 0 1.27 180) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(C7-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module vco-sma:SOT-343 placed (layer B.Cu) (tedit 56EABF48)
    (at 31.115 28.067)
    (descr SOT353)
    (attr smd)
    (fp_text reference Q2 (at 0 -0.127 270) (layer B.SilkS))
    (fp_text value BFP420 (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.016 0.635) (size 0.508 0.3048) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at -1.016 -0.485) (size 0.508 0.6048) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(L2-Pad1)"))
    (pad 2 smd rect (at 1.016 0.635) (size 0.508 0.3048) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(L2-Pad1)"))
    (pad 3 smd rect (at 1.016 -0.635) (size 0.508 0.3048) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-353.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.07000000000000001 0.09 0.08))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering placed (layer F.Cu) (tedit 56EABF0D)
    (at 34.671 22.733 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at -2.54 0 270) (layer F.SilkS))
    (fp_text value 15pF (at 0.955 -1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering placed (layer B.Cu) (tedit 56EABF23)
    (at 28.829 25.019 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at -0.762 -1.27 180) (layer B.SilkS))
    (fp_text value 3pF (at 0.635 1.27 180) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C2-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering placed (layer F.Cu) (tedit 56EABEE9)
    (at 33.147 22.733 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C4 (at -2.54 0 270) (layer F.SilkS))
    (fp_text value 3pF (at -0.95 1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering placed (layer F.Cu) (tedit 56EABEA3)
    (at 34.29 27.178 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C5 (at -1.143 -1.016 270) (layer F.SilkS))
    (fp_text value 15pF (at -1.27 1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C5-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:SOD-323 placed (layer B.Cu) (tedit 56EABF60)
    (at 36.195 22.86 270)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D1 (at 0.127 -1.27 270) (layer B.SilkS))
    (fp_text value VARICAP (at 0.215 0.635 270) (layer B.Fab))
    (pad 1 smd rect (at -1.055 0 270) (size 0.59 0.45) (layers B.Cu B.Paste B.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 1.055 0 270) (size 0.59 0.45) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(D1-Pad2)"))
  )
  (module Diodes_SMD:SOD-323 placed (layer B.Cu) (tedit 56EABF5A)
    (at 36.195 26.67 90)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D2 (at 0 1.27 90) (layer B.SilkS))
    (fp_text value VARICAP (at 0 -0.635 90) (layer B.Fab))
    (pad 1 smd rect (at -1.055 0 90) (size 0.59 0.45) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(C5-Pad2)"))
    (pad 2 smd rect (at 1.055 0 90) (size 0.59 0.45) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(D1-Pad2)"))
  )
  (module Resistors_SMD:R_0603_HandSoldering placed (layer B.Cu) (tedit 56EABF13)
    (at 32.893 21.463 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference L1 (at 0 -1.27 180) (layer B.SilkS))
    (fp_text value 5nH (at 0.635 1.27 180) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 14 +5V))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering placed (layer B.Cu) (tedit 56EABE0A)
    (at 28.745 37.465)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference L2 (at -0.17 1.27) (layer B.SilkS))
    (fp_text value 4.7nH (at -1.27 1.27) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(L2-Pad1)"))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(C3-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01 placed (layer F.Cu) (tedit 56F33A92)
    (at 39.37 28.575)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference Tune (at 1.905 0 90) (layer F.SilkS))
    (fp_text value Tuning (at 1.905 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(P1-Pad1)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 placed (layer F.Cu) (tedit 56F33A7A)
    (at 39.37 23.495 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference Power (at -1.905 1.27 270) (layer F.SilkS))
    (fp_text value Power (at -1.905 1.27 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 Earth))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 +5V))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering placed (layer F.Cu) (tedit 56EABF1B)
    (at 36.449 22.733 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 2.54 0 90) (layer F.SilkS))
    (fp_text value 10k (at -0.17 1.27 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 Earth))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering placed (layer B.Cu) (tedit 56EABF4E)
    (at 27.813 28.194 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at 0.127 -1.27 90) (layer B.SilkS))
    (fp_text value 3k (at -0.465 -1.27 90) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(C7-Pad1)"))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C2-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering placed (layer F.Cu) (tedit 56EABE7E)
    (at 30.48 37 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 2.37 0 270) (layer F.SilkS))
    (fp_text value 100R (at 0.805 1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 Earth))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering placed (layer B.Cu) (tedit 56EABED5)
    (at 35.476 29.21 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at 0.043 -1.397 180) (layer B.SilkS))
    (fp_text value 10k (at -0.635 -1.27 180) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(P1-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(D1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering placed (layer F.Cu) (tedit 56EABEDF)
    (at 36.322 27.178 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R6 (at -1.143 -1.143 270) (layer F.SilkS))
    (fp_text value 10k (at 0.635 -1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 Earth))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C5-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module vco-sma:SOT-343 placed (layer B.Cu) (tedit 56EABF32)
    (at 29.21 22.352)
    (descr SOT353)
    (attr smd)
    (fp_text reference Q1 (at 0 -0.127 180) (layer B.SilkS))
    (fp_text value BFP420 (at 0 -1.905 270) (layer B.Fab))
    (pad 1 smd rect (at -1.016 0.635) (size 0.508 0.3048) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C2-Pad2)"))
    (pad 2 smd rect (at -1.016 -0.485) (size 0.508 0.6048) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(L2-Pad1)"))
    (pad 2 smd rect (at 1.016 0.635) (size 0.508 0.3048) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(L2-Pad1)"))
    (pad 3 smd rect (at 1.016 -0.635) (size 0.508 0.3048) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-353.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.07000000000000001 0.09 0.08))
      (rotate (xyz 0 0 90))
    )
  )
  (module vco-sma:SMA locked (layer F.Cu) (tedit 56F3EB82)
    (at 37.465 35.08502 270)
    (tags "SMA Connector")
    (fp_text reference J1 (at 0 1.905 270) (layer F.SilkS))
    (fp_text value SMA (at 0 -4.445 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(C6-Pad1)"))
    (pad 2 thru_hole circle (at 2.70002 -2.70002 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 6 Earth))
    (pad 2 thru_hole circle (at -2.70002 -2.70002 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 6 Earth))
    (pad 2 thru_hole circle (at -2.70002 2.70002 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 6 Earth))
    (pad 2 thru_hole circle (at 2.70002 2.70002 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 6 Earth))
    (model connectors/sma.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz -90 0 -90))
    )
  )
  (gr_text "© Tim Clark 2016" (at 26.543 22.479 270) (layer F.SilkS))
  (gr_text "VCO V1.0\n500MHz - 1GHz" (at 28.321 22.225 270) (layer F.SilkS))
  (dimension 17.78 (width 0.3) (layer F.Fab)
    (gr_text "17.780 mm" (at 33.655 43.895) (layer F.Fab))
    (feature1 (pts (xy 42.545 40.005) (xy 42.545 45.245)))
    (feature2 (pts (xy 24.765 40.005) (xy 24.765 45.245)))
    (crossbar (pts (xy 24.765 42.545) (xy 42.545 42.545)))
    (arrow1a (pts (xy 42.545 42.545) (xy 41.418496 43.131421)))
    (arrow1b (pts (xy 42.545 42.545) (xy 41.418496 41.958579)))
    (arrow2a (pts (xy 24.765 42.545) (xy 25.891504 43.131421)))
    (arrow2b (pts (xy 24.765 42.545) (xy 25.891504 41.958579)))
  )
  (dimension 21.59 (width 0.3) (layer F.Fab)
    (gr_text "21.590 mm" (at 20.875 29.21 270) (layer F.Fab))
    (feature1 (pts (xy 24.765 40.005) (xy 19.525 40.005)))
    (feature2 (pts (xy 24.765 18.415) (xy 19.525 18.415)))
    (crossbar (pts (xy 22.225 18.415) (xy 22.225 40.005)))
    (arrow1a (pts (xy 22.225 40.005) (xy 21.638579 38.878496)))
    (arrow1b (pts (xy 22.225 40.005) (xy 22.811421 38.878496)))
    (arrow2a (pts (xy 22.225 18.415) (xy 21.638579 19.541504)))
    (arrow2b (pts (xy 22.225 18.415) (xy 22.811421 19.541504)))
  )
  (gr_line (start 24.765 40.005) (end 24.765 18.415) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 42.545 40.005) (end 24.765 40.005) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 42.545 18.415) (end 42.545 40.005) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 24.765 18.415) (end 42.545 18.415) (layer Edge.Cuts) (width 0.15))
  (zone (net 6) (net_name Earth) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 42.545 40.005) (xy 24.765 40.005) (xy 24.765 18.415) (xy 42.545 18.415) (xy 42.545 29.845)
      )
    )
  )
  (zone (net 6) (net_name Earth) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 42.545 40.005) (xy 24.765 40.005) (xy 24.765 18.415) (xy 42.545 18.415) (xy 42.545 28.575)
      )
    )
  )
)
