(kicad_pcb (version 4) (host pcbnew 4.0.1-stable)
  (general
    (links 42)
    (no_connects 2)
    (area 13.894999 13.894999 52.361441 42.298686)
    (thickness 1.6)
    (drawings 6)
    (tracks 106)
    (zones 0)
    (modules 25)
    (nets 15)
  )
  (page A4)
  (layers
    (0 F.Cu signal hide)
    (31 B.Cu signal hide)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user hide)
    (37 F.SilkS user hide)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user hide)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 0.5 0.5)
    (mod_text_width 0.075)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (grid_origin 12.065 12.065)
    (visible_elements FFFFC461)
    (pcbplotparams
      (layerselection 0x00010_80000000)
      (usegerberextensions false)
      (excludeedgelayer false)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk true)
      (subtractmaskfromsilk false)
      (outputformat 5)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 "Net-(C1-Pad2)")
  (net 3 "Net-(C2-Pad1)")
  (net 4 "Net-(C2-Pad2)")
  (net 5 "Net-(C3-Pad1)")
  (net 6 Earth)
  (net 7 "Net-(C4-Pad1)")
  (net 8 "Net-(C5-Pad2)")
  (net 9 "Net-(C6-Pad1)")
  (net 10 "Net-(C7-Pad1)")
  (net 11 "Net-(D1-Pad2)")
  (net 12 "Net-(L2-Pad1)")
  (net 13 "Net-(P1-Pad1)")
  (net 14 +5V)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net Earth)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C5-Pad2)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(L2-Pad1)")
    (add_net "Net-(P1-Pad1)")
  )
  (module Resistors_SMD:R_0603_HandSoldering placed (layer B.Cu) (tedit 56EABF3A)
    (at 26.67 22.86 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference L3 (at -0.635 1.27 180) (layer B.SilkS))
    (fp_text value 5nH (at 0.635 1.27 180) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 14 +5V))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering placed (layer B.Cu) (tedit 56EABEA1)
    (at 29.21 31.92 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R7 (at -1.44 1.27 270) (layer B.SilkS))
    (fp_text value 100R (at 0.465 1.27 270) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 14 +5V))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(C7-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering placed (layer B.Cu) (tedit 56EABDF2)
    (at 29.21 36.365 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R8 (at -0.17 -1.27 270) (layer B.SilkS))
    (fp_text value 3k (at 1.1 -1.27 270) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(C7-Pad1)"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 6 Earth))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering placed (layer B.Cu) (tedit 56EABE93)
    (at 26.67 30.48 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at -1.27 1.27 270) (layer B.SilkS))
    (fp_text value 3k (at 0 1.27 270) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(C7-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module vco-sma:SOT-343 placed (layer B.Cu) (tedit 56EABF48)
    (at 22.86 23.495)
    (descr SOT353)
    (attr smd)
    (fp_text reference Q2 (at 0 1.905 270) (layer B.SilkS))
    (fp_text value BFP420 (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.016 0.635) (size 0.508 0.3048) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at -1.016 -0.485) (size 0.508 0.6048) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(L2-Pad1)"))
    (pad 2 smd rect (at 1.016 0.635) (size 0.508 0.3048) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(L2-Pad1)"))
    (pad 3 smd rect (at 1.016 -0.635) (size 0.508 0.3048) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-353.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.07000000000000001 0.09 0.08))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering placed (layer B.Cu) (tedit 56EABF0D)
    (at 31.435 19.685 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at -0.95 1.27 180) (layer B.SilkS))
    (fp_text value 15pF (at 0.955 1.27 180) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering placed (layer B.Cu) (tedit 56EABF23)
    (at 24.13 20.955 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at -0.635 1.27 180) (layer B.SilkS))
    (fp_text value 3pF (at 0.635 1.27 180) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C2-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering placed (layer B.Cu) (tedit 56EABE0E)
    (at 24.45 37.465 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at -0.95 -1.27 180) (layer B.SilkS))
    (fp_text value 1.7pF (at 0.955 -1.27 180) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 6 Earth))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering placed (layer B.Cu) (tedit 56EABEE9)
    (at 26.67 25.72 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C4 (at 0.955 -1.27 90) (layer B.SilkS))
    (fp_text value 3pF (at -0.95 -1.27 90) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering placed (layer B.Cu) (tedit 56EABEA3)
    (at 31.75 31.75 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C5 (at 0.635 -1.27 90) (layer B.SilkS))
    (fp_text value 15pF (at -1.27 -1.27 90) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(C5-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering placed (layer B.Cu) (tedit 56EABEA9)
    (at 33.02 35.56 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C6 (at -1.27 -1.27 180) (layer B.SilkS))
    (fp_text value 4.7pF (at 0.635 -1.27 180) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(C6-Pad1)"))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:c_elec_6.3x5.7 placed (layer B.Cu) (tedit 56EABEF8)
    (at 21.59 31.115 90)
    (descr "SMT capacitor, aluminium electrolytic, 6.3x5.7")
    (attr smd)
    (fp_text reference C7 (at 0 -0.635 90) (layer B.SilkS))
    (fp_text value 10uF (at 0 1.27 90) (layer B.Fab))
    (pad 1 smd rect (at 2.75082 0 90) (size 3.59918 1.6002) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(C7-Pad1)"))
    (pad 2 smd rect (at -2.75082 0 90) (size 3.59918 1.6002) (layers B.Cu B.Paste B.Mask)
      (net 6 Earth))
    (model Capacitors_SMD.3dshapes/c_elec_6.3x5.7.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:SOD-323 placed (layer B.Cu) (tedit 56EABF60)
    (at 31.75 22.645 270)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D1 (at 0.215 -0.635 270) (layer B.SilkS))
    (fp_text value VARICAP (at 0.215 0.635 270) (layer B.Fab))
    (pad 1 smd rect (at -1.055 0 270) (size 0.59 0.45) (layers B.Cu B.Paste B.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 1.055 0 270) (size 0.59 0.45) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(D1-Pad2)"))
  )
  (module Diodes_SMD:SOD-323 placed (layer B.Cu) (tedit 56EABF5A)
    (at 31.75 27.305 90)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D2 (at 0 0.635 90) (layer B.SilkS))
    (fp_text value VARICAP (at 0 -0.635 90) (layer B.Fab))
    (pad 1 smd rect (at -1.055 0 90) (size 0.59 0.45) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(C5-Pad2)"))
    (pad 2 smd rect (at 1.055 0 90) (size 0.59 0.45) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(D1-Pad2)"))
  )
  (module Resistors_SMD:R_0603_HandSoldering placed (layer B.Cu) (tedit 56EABF13)
    (at 26.67 19.05 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference L1 (at -1.27 1.27 180) (layer B.SilkS))
    (fp_text value 5nH (at 0.635 1.27 180) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 14 +5V))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering placed (layer B.Cu) (tedit 56EABE0A)
    (at 20.32 37.465)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference L2 (at 0.635 1.27) (layer B.SilkS))
    (fp_text value 4.7nH (at -1.27 1.27) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(L2-Pad1)"))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(C3-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01 placed (layer F.Cu) (tedit 56EABECA)
    (at 39.37 28.575)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at 0 -5.1) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 3.81 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(P1-Pad1)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 placed (layer F.Cu) (tedit 56EABECD)
    (at 39.37 23.495 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P3 (at -1.905 1.27 180) (layer F.SilkS))
    (fp_text value CONN_01X02 (at -3.81 0 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 Earth))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 +5V))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering placed (layer B.Cu) (tedit 56EABF1B)
    (at 29.845 22.69 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 1.1 -1.27 90) (layer B.SilkS))
    (fp_text value 10k (at -0.17 -1.27 90) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 6 Earth))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering placed (layer B.Cu) (tedit 56EABF4E)
    (at 20.32 23.03 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at 0.805 -1.27 90) (layer B.SilkS))
    (fp_text value 3k (at -0.465 -1.27 90) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(C7-Pad1)"))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C2-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering placed (layer B.Cu) (tedit 56EABE7E)
    (at 27.305 36.365 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 2.71 -1.27 90) (layer B.SilkS))
    (fp_text value 100R (at 0.805 -1.27 90) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 6 Earth))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering placed (layer B.Cu) (tedit 56EABED5)
    (at 34.29 27.305 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at 1.27 -1.27 90) (layer B.SilkS))
    (fp_text value 10k (at -0.635 -1.27 90) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(P1-Pad1)"))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(D1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering placed (layer B.Cu) (tedit 56EABEDF)
    (at 29.845 27.305 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R6 (at -1.27 1.27 270) (layer B.SilkS))
    (fp_text value 10k (at 0.635 1.27 270) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 6 Earth))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(C5-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module vco-sma:SOT-343 placed (layer B.Cu) (tedit 56EABF32)
    (at 22.86 18.415)
    (descr SOT353)
    (attr smd)
    (fp_text reference Q1 (at 0 0 270) (layer B.SilkS))
    (fp_text value BFP420 (at 0 -1.905 270) (layer B.Fab))
    (pad 1 smd rect (at -1.016 0.635) (size 0.508 0.3048) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C2-Pad2)"))
    (pad 2 smd rect (at -1.016 -0.485) (size 0.508 0.6048) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(L2-Pad1)"))
    (pad 2 smd rect (at 1.016 0.635) (size 0.508 0.3048) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(L2-Pad1)"))
    (pad 3 smd rect (at 1.016 -0.635) (size 0.508 0.3048) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-353.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.07000000000000001 0.09 0.08))
      (rotate (xyz 0 0 90))
    )
  )
  (module vco-sma:SMA locked (layer F.Cu) (tedit 56EABEAD)
    (at 39.37 35.56 270)
    (tags "SMA Connector")
    (fp_text reference J1 (at 0 5.08 270) (layer F.SilkS))
    (fp_text value SMA-vco (at 0 -4.445 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(C6-Pad1)"))
    (pad 2 thru_hole circle (at 2.70002 -2.70002 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 6 Earth))
    (pad 2 thru_hole circle (at -2.70002 -2.70002 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 6 Earth))
    (pad 2 thru_hole circle (at -2.70002 2.70002 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 6 Earth))
    (pad 2 thru_hole circle (at 2.70002 2.70002 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 6 Earth))
    (model connectors/sma.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz -90 0 -90))
    )
  )
  (gr_line (start 13.97 40.64) (end 15.24 40.64) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 15.875 13.97) (end 15.875 40.64) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 44.45 15.875) (end 13.97 15.875) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 44.45 15.24) (end 44.45 13.97) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 15.24 40.64) (end 44.45 40.64) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 44.45 40.64) (end 44.45 15.24) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 6) (net_name Earth) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 44.45 40.64) (xy 15.875 40.64) (xy 15.875 15.875) (xy 44.45 15.875) (xy 44.45 40.64)
      )
    )
  )
)
